/* ROM version variables for esp32s3
 *
 * These addresses should be compatible with any ROM version for this chip.
 *
 * THIS FILE WAS AUTOMATICALLY GENERATED. DO NOT EDIT.
 */
_rom_chip_id = 0x40000570;
_rom_eco_version = 0x40000574;
